{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["报价表"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"报价表","index":0,"n_rows":86,"n_cols":12,"rows_kept":86,"merged":[[0,0,0,11],[1,0,1,11],[2,0,2,11],[3,0,3,11],[4,0,4,11],[5,0,6,0],[5,1,5,7],[5,8,5,11],[7,0,14,0],[7,2,14,2],[7,5,14,5],[7,6,14,6],[7,7,14,7],[9,1,11,1],[12,1,14,1],[15,0,15,11],[16,0,17,0],[16,1,16,7],[16,8,16,11],[18,0,27,0],[18,1,19,1],[18,6,27,6],[18,7,27,7],[21,1,23,1],[24,1,27,1],[28,0,28,11],[29,0,30,0],[29,1,29,7],[29,8,29,11],[31,0,34,0],[31,1,32,1],[31,6,40,6],[31,7,34,7],[31,11,40,11],[33,1,34,1],[35,0,40,0],[35,1,40,1],[35,2,40,2],[35,7,40,7],[43,0,43,11],[44,0,45,0],[44,1,44,7],[44,8,44,11],[46,0,49,0],[46,6,49,6],[46,7,49,7],[50,0,50,11],[51,0,52,0],[51,1,51,7],[51,8,51,11],[53,0,80,0],[53,6,80,6],[53,7,80,7],[54,1,55,1],[54,2,55,2],[56,1,57,1],[58,1,59,1],[77,1,78,1],[79,1,80,1],[81,0,81,11],[82,0,82,7]],"flags":["formulas_cached_only"]}
["主材招标采购报价单招标编号：TYZB-2020-051"]
["招标单位：山东铁鹰建设工程有限公司           联系人：李强 马飞   0538-6629816"]
["投标地址：tieyingzhaobiao@139.com         开标时间：2020-12-15 11:00"]
["报价单位（盖章）：                         联系人："]
["标一"]
["类别","招标信息",{"$nulls":6},"报价信息"]
[null,"材料名称","材质","型号","单位","数量","卸货地址","具体要求","价格","下差范围","产地（厂家）","其他情况"]
[null,"3mm花纹板",null,"1.25*6","页","80T",null,"板宽1.508以上、板面平整无划痕 、对角线尺寸达标"]
[null,"3mm面板",null,"1.25*6","页"]
[null,"4mm板",null,"1.5*6","页"]
[{"$nulls":3},"1.25*特尺","页"]
[{"$nulls":3},"2*特尺","页"]
[null,"5-12mm开平板",null,"2.01*特尺","页"]
[{"$nulls":3},"1.25*特尺","页"]
[{"$nulls":3},"1.51*特尺","页",{"$nulls":5}," "]
["标二"]
["类别","招标信息",{"$nulls":6},"报价信息"]
[null,"材料名称","材质","型号","单位","数量","卸货地址","具体要求","价格","下差范围","产地（厂家）","其他情况"]
["带钢","8mm带钢","Q235","50*6","支",4,"分厂、总厂","不允许有圆弧边"]
[null,null,"Q235","80*6","支"]
[null,"6mm带钢","Q235","70*6","支"]
[null,"10mm带钢","Q235","50*5","支",22]
[null,null,"Q235","100*6","支",40]
[null,null,"Q235","80*6","支",22]
[null,"12mm带钢","Q235","100*6","支"]
[null,null,"Q235","150*6","支",1]
[null,null,"Q235","80*6","支",174]
[null,null,"Q235","130*6","支",8]
["标三"]
["类别","招标信息",{"$nulls":6},"报价信息"]
[null,"材料名称","材质","型号","单位","数量","卸货地址","具体要求","价格","下差范围","产地（厂家）","其他情况"]
["复合板","5+1mm不锈钢板（201）",304,"1.51*4.25","页",0," ","油抛光亮、表面平整无划痕、无麻点",{"$nulls":3},"付款条件可以要求30%预付款定货，货到付全款"]
[null,null,304,"1.51*3.33","页",0]
[null,"5+1mm不锈钢板（304）",304,"1.51*2.06","页",18]
[null,null,304,"1.51*2.1","页",18]
["不锈钢","8mm不锈钢板（201）",201,"1.51*3.82","页",24,null,"油抛、表面平整无划痕、无麻点"]
[{"$nulls":3},"1.51*3.04","页",2]
[{"$nulls":3},"1.51*2.53","页",44]
[{"$nulls":3},"1.51*2.34","页",3]
[{"$nulls":3},"1.51*2.56","页",2]
[{"$nulls":3},"1.51*2.39","页",0]
[]
[]
["标四"]
["类别","招标信息",{"$nulls":6},"报价信息"]
[null,"材料名称","材质","型号","单位","数量","卸货地址","具体要求","价格","下差范围","产地（厂家）","其他情况"]
["中板","16mm普板","Q235","2.2*10","页",null,"分厂、总厂","有现货 "]
[null,"10mm普板","Q235","2.2*10","页"]
[null,"12mm普板","Q235","2.2*10","页"," "]
[null,"20mm普板","Q235","2.2*10","页"]
["标五"]
["类别","招标信息",{"$nulls":6},"报价信息"]
[null,"材料名称","材质","型号","单位","数量","卸货地址","具体要求","价格","下差范围","产地（厂家）","其他情况"]
["型材","【5","Q235","6米","支",13,"分厂、总厂","下差100以内，越小越好、角钢角度为必须直角；槽钢角度误差3mm内，禁止供辽钢货"]
[null,"【8","Q235","6米","支",494]
[{"$nulls":3},"9米","支"]
[null,"【10","Q235","9米","支"]
[null,null,"Q235","6米","支",257]
[null,"【12","Q235","6米","支",31]
[null,null,"Q235","9米","支"]
[null,"【16A","Q235","9米","支"]
[null,"【16B","Q235","9米","支",61]
[null,"【14A","Q235","9米","支"]
[null,"4.5mm粗钢板网","Q235","2*4米","页",95,{"$nulls":5},"孔距10cm"]
[null,"30A工","Q235","12米","支",15]
[null,"76*6无缝","Q235","米","米"]
[null,"48*3.5无缝","Q235","米","米",80]
[null,"219*6无缝","Q235","米","米",25]
[null,"22*2.5管子","Q235","米","米",28]
[null,"32*3管子","Q235","6米","支",460]
[null,"42*3管子","Q235","6米","支",35]
[null,"口40*2","Q235","6米","支",2]
[null,"口30*3","Q235","6米","支",40]
[null,"口50*3","Q235","6米","支",185]
[null,"口30*2","Q235","6米","支",110]
[null,"L75*8","Q235","6米","支",17]
[null,"L50*5","Q235","6米","支",156]
[null,"L80*80*8","Q235","6米","支",18]
[null,null,"Q235","9米","支"]
[null,"L100*100*10","Q235","9米","支",3]
[null,null,"Q235","6米","支"]
["以上报价内容为（不可更改无二次报价机会）：1、国标货、泰安满庄提货或送到、过磅含税价；2、付款方式为货到需方收货后付款；3、收货方式按照需方过磅重量（磅差千分之一以内）电汇结算；4、结算前需提供材质书、购销合同、收据、发票等相关凭据；5、供货周期为三日内到全；6、本次报价请各报价单位按照自己公司优势选着性报价，同时允许多个包件同时报价，我公司按照单项低价选择中标。"]
["本次报价有效期为：       日内（报价单位必填）       ",{"$nulls":7},"报价单位（盖章）："]
[{"$nulls":8},"报价时间："]
[{"$nulls":8},"报价人："]
[{"$nulls":8},"联系电话："]