{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["报价表"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"报价表","index":0,"n_rows":86,"n_cols":12,"rows_kept":86,"merged":[[0,0,0,11],[1,0,1,11],[2,0,2,11],[3,0,3,11],[4,0,4,11],[5,0,6,0],[5,1,5,7],[5,8,5,11],[7,0,10,0],[7,2,10,2],[7,5,10,5],[7,6,10,6],[7,7,10,7],[8,1,10,1],[11,0,11,11],[12,0,13,0],[12,1,12,7],[12,8,12,11],[14,0,23,0],[14,1,15,1],[14,6,23,6],[14,7,23,7],[17,1,19,1],[20,1,23,1],[24,0,24,11],[25,0,26,0],[25,1,25,7],[25,8,25,11],[27,0,33,0],[27,1,30,1],[27,6,37,6],[27,7,33,7],[27,11,37,11],[31,1,33,1],[34,0,37,0],[34,1,37,1],[34,2,37,2],[34,7,37,7],[40,0,40,11],[41,0,42,0],[41,1,41,7],[41,8,41,11],[43,0,46,0],[43,6,46,6],[43,7,46,7],[47,0,47,11],[48,0,49,0],[48,1,48,7],[48,8,48,11],[50,0,80,0],[50,6,80,6],[50,7,80,7],[52,1,53,1],[52,2,53,2],[54,1,55,1],[56,1,57,1],[77,1,78,1],[79,1,80,1],[81,0,81,11],[82,0,82,7]],"flags":["formulas_cached_only"]}
["主材招标采购报价单招标编号：TYZB-2021-001"]
["招标单位：山东铁鹰建设工程有限公司           联系人：李强 马飞   0538-6629816"]
["投标地址：tieyingzhaobiao@139.com         开标时间：2021-1-5 11:00"]
["报价单位（盖章）：                         联系人："]
["标一"]
["类别","招标信息",{"$nulls":6},"报价信息"]
[null,"材料名称","材质","型号","单位","数量","卸货地址","具体要求","价格","下差范围","产地（厂家）","其他情况"]
[null,"3mm花纹板",null,"1.25*6","页","50T",null,"板宽1.508以上、板面平整无划痕 、对角线尺寸达标"]
[null,"5-12mm开平板",null,"2.01*特尺","页"]
[{"$nulls":3},"1.25*特尺","页"]
[{"$nulls":3},"1.51*特尺","页",{"$nulls":5}," "]
["标二"]
["类别","招标信息",{"$nulls":6},"报价信息"]
[null,"材料名称","材质","型号","单位","数量","卸货地址","具体要求","价格","下差范围","产地（厂家）","其他情况"]
["带钢","8mm带钢","Q235","50*6","支",null,"分厂、总厂","不允许有圆弧边"]
[null,null,"Q235","80*6","支"]
[null,"6mm带钢","Q235","70*6","支"]
[null,"10mm带钢","Q235","63*6","支",84]
[null,null,"Q235","100*6","支",35]
[null,null,"Q235","80*6","支",60]
[null,"12mm带钢","Q235","100*6","支",60]
[null,null,"Q235","120*6","支",69]
[null,null,"Q235","80*6","支",35]
[null,null,"Q235","140*6","支",69]
["标三"]
["类别","招标信息",{"$nulls":6},"报价信息"]
[null,"材料名称","材质","型号","单位","数量","卸货地址","具体要求","价格","下差范围","产地（厂家）","其他情况"]
["复合板","5+1mm不锈钢板（304）",304,"1.51*3.34","页",7," ","油抛光亮、表面平整无划痕、无麻点",{"$nulls":3},"付款条件可以要求30%预付款定货，货到付全款"]
[null,null,304,"1.51*3.48","页",1]
[null,null,304,"1.51*3.59","页",5]
[null,null,304,"1.51*3.65","页",5]
[null,"6+2mm不锈钢板（304）",304,"1.51*2.57","页"]
[null,null,304,"1.51*2.89","页"]
[null,null,304,"1.51*3.19","页"]
["不锈钢","6mm不锈钢板",201,"1.51*4.05","页",4,null,"油抛、表面平整无划痕、无麻点"]
[{"$nulls":3},"1.51*5.24","页",1]
[{"$nulls":3},"1.51*3.56","页",1]
[{"$nulls":3},"3.23*1.51","页",0]
[]
[]
["标四"]
["类别","招标信息",{"$nulls":6},"报价信息"]
[null,"材料名称","材质","型号","单位","数量","卸货地址","具体要求","价格","下差范围","产地（厂家）","其他情况"]
["中板","16mm普板","Q235","2.2*10","页",null,"分厂、总厂","有现货 "]
[null,"10mm普板","Q235","2.2*10","页"]
[null,"12mm普板","Q235","2.2*10","页"]
[null,"20mm普板","Q235","2.2*10","页"]
["标五"]
["类别","招标信息",{"$nulls":6},"报价信息"]
[null,"材料名称","材质","型号","单位","数量","卸货地址","具体要求","价格","下差范围","产地（厂家）","其他情况"]
["型材","【5","Q235","6米","支",3,"分厂、总厂","下差100以内，越小越好、角钢角度为必须直角；槽钢角度误差3mm内，禁止供辽钢货"]
[null,"【6.3","Q235","6米","支",265]
[null,"【8","Q235","6米","支",82]
[{"$nulls":3},"9米","支"]
[null,"【10","Q235","9米","支"]
[null,null,"Q235","6米","支",154]
[null,"【12","Q235","6米","支",56]
[null,null,"Q235","9米","支"]
[null,"【14A","Q235","6米","支",539]
[null,"【14B","Q235","6米","支",34]
[null,"【16A","Q235","9米","支",198]
[null,"【20A","Q235","12米","支",12]
[null,"工32A","Q235","12米","支",54,{"$nulls":5}," "]
[null,"工10","Q235","6米","支",12]
[null,"工16","Q235","9米","支",2]
[null,"工20B","Q235","12米","支",2]
[null,"H200*204*12","Q235","12米","支",30]
[null,"22*3管","Q235","米","米",21]
[null,"48*3.5无缝","Q235","6米","支",14]
[null,"76*6无缝","Q235","米","米",36]
[null,"42*3管","Q235","6米","支",1]
[null,"108*5无缝","Q235","6米","支",32]
[null,"口40*2","Q235","6米","支",3]
[null,"口30*2","Q235","6米","支",66]
[null,"L110*70*8","Q235","6米","支"]
[null,"L50*5","Q235","6米","支",81]
[null,"L63*6","Q235","6米","支",265]
[null,"L80*80*8","Q235","6米","支"]
[null,null,"Q235","9米","支"]
[null,"L100*100*10","Q235","9米","支"]
[null,null,"Q235","6米","支"]
["以上报价内容为（不可更改无二次报价机会）：1、国标货、泰安满庄提货或送到、过磅含税价；2、付款方式为货到需方收货后付款；3、收货方式按照需方过磅重量（磅差千分之一以内）电汇结算；4、结算前需提供材质书、购销合同、收据、发票等相关凭据；5、供货周期为三日内到全；6、本次报价请各报价单位按照自己公司优势选着性报价，同时允许多个包件同时报价，我公司按照单项低价选择中标。"]
["本次报价有效期为：       日内（报价单位必填）       ",{"$nulls":7},"报价单位（盖章）："]
[{"$nulls":8},"报价时间："]
[{"$nulls":8},"报价人："]
[{"$nulls":8},"联系电话："]