{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["报价表"],"read":"whole","date_system":"1900"}

{"sheet":"报价表","index":0,"n_rows":85,"n_cols":12,"rows_kept":85,"merged":[[0,0,0,11],[1,0,1,11],[2,0,2,11],[3,0,3,11],[4,0,4,11],[5,0,6,0],[5,1,5,7],[5,8,5,11],[7,0,10,0],[7,2,10,2],[7,5,10,5],[7,6,10,6],[7,7,10,7],[8,1,10,1],[11,0,11,11],[12,0,13,0],[12,1,12,7],[12,8,12,11],[14,0,25,0],[14,1,16,1],[14,6,25,6],[14,7,25,7],[18,1,20,1],[21,1,25,1],[26,0,26,11],[27,0,28,0],[27,1,27,7],[27,8,27,11],[29,0,32,0],[29,1,31,1],[29,6,34,6],[29,7,34,7],[29,11,34,11],[33,0,34,0],[33,1,34,1],[33,2,34,2],[35,0,35,11],[36,0,37,0],[36,1,36,7],[36,8,36,11],[38,0,40,0],[38,6,40,6],[38,7,40,7],[41,0,41,11],[42,0,43,0],[42,1,42,7],[42,8,42,11],[44,0,79,0],[44,6,79,6],[44,7,79,7],[46,1,47,1],[46,2,47,2],[48,1,49,1],[50,1,51,1],[52,1,53,1],[76,1,77,1],[78,1,79,1],[80,0,80,11],[81,0,81,7]]}
["主材招标采购报价单招标编号：TYZB-2021-052"]
["招标单位：山东铁鹰建设工程有限公司           联系人：李强 马飞   0538-6629816"]
["投标地址：tieyingzhaobiao@139.com         开标时间：2021-9-24 11:00"]
["报价单位（盖章）：                         联系人："]
["标一"]
["类别","招标信息",{"$nulls":6},"报价信息"]
[null,"材料名称","材质","型号","单位","数量","卸货地址","具体要求","价格","下差范围","产地（厂家）","其他情况"]
[null,"3mm花纹板",null,"1.25*6","页",150,null,"板宽1.508以上、板面平整无划痕 、对角线尺寸达标"]
[null,"5-12mm开平板",null,"2.01*特尺","页"]
[{"$nulls":3},"1.25*特尺","页"]
[{"$nulls":3},"1.51*特尺","页",{"$nulls":5}," "]
["标二"]
["类别","招标信息",{"$nulls":6},"报价信息"]
[null,"材料名称","材质","型号","单位","数量","卸货地址","具体要求","价格","下差范围","产地（厂家）","其他情况"]
["带钢","8mm带钢","Q235","50*6","支",null,"分厂、总厂","不允许有圆弧边"]
[null,null,"Q235","63*6","支"]
[null,null,"Q235","140*6","支"]
[null,"6mm带钢","Q235","49*6","支"]
[null,"10mm带钢","Q235","80*6","支",15]
[null,null,"Q235","80*9","支"," "]
[null,null,"Q235","150*6","支"]
[null,"12mm带钢","Q235","80*6","支",{"$f":"69+26+82+48+4+34+30+2","v":295}]
[null,null,"Q235","80*9","支",{"$f":"29+49","v":78}]
[null,null,"Q235","120*6","支",126]
[null,null,"Q235","100*6","支",42]
[null,null,"Q235","160*6","支",42]
["标三"]
["类别","招标信息",{"$nulls":6},"报价信息"]
[null,"材料名称","材质","型号","单位","数量","卸货地址","具体要求","价格","下差范围","产地（厂家）","其他情况"]
["复合板","5+1mm不锈钢板复合板（304）",304,"1.23*6","页"," "," ","油抛光亮、表面平整无划痕、无麻点"]
[null,null,304,"1.51*n","页"," "]
[null,null,304,"2.01*n","页"," "]
[null,"6mm不锈钢板复合板（304）",304,"1.51*3.73","页"]
["不锈钢板","6mm不锈钢板（201）",201,"1.51*5.74","页"]
[{"$nulls":3},"1.51*3.2","页"]
["标四"]
["类别","招标信息",{"$nulls":6},"报价信息"]
[null,"材料名称","材质","型号","单位","数量","卸货地址","具体要求","价格","下差范围","产地（厂家）","其他情况"]
["中板","10mm普板","Q235","2.2*10","页"," ","分厂、总厂","有现货 "]
[null,"20mm锰板","Q235","2.2*10","页",1]
[null,"16-20mm普板","Q235","2.2*10","页"," "]
["标五"]
["类别","招标信息",{"$nulls":6},"报价信息"]
[null,"材料名称","材质","型号","单位","数量","卸货地址","具体要求","价格","下差范围","产地（厂家）","其他情况"]
["型材","【5","Q235","6米","支",null,"分厂、总厂","下差100以内，越小越好、角钢角度为必须直角；槽钢角度误差3mm内，禁止供辽钢货"]
[null,"【6.3","Q335","6米","支",320]
[null,"【8","Q235","6米","支",{"$f":"33+27+27+100+170+61+158","v":576}]
[{"$nulls":3},"9米","支",{"$f":"126+86","v":212}]
[null,"【10","Q235","9米","支",{"$f":"64+48","v":112}]
[null,null,"Q235","6米","支",{"$f":"165+32+36+36+32","v":301}]
[null,"【12","Q235","6米","支",{"$f":"570+10+117+77","v":774}]
[null,null,"Q235","9米","支"]
[null,"【14A","Q235","6米","支",48]
[null,null,"Q235","9米","支"]
[null,"【16B","Q235","9米","支",{"$f":"54+49","v":103}]
[null,"【18B","Q235","12米","支"]
[null,"【25B","Q235","12米","支"]
[null,"【28A","Q235","12米","支",7]
[null,"【20a","Q235","12米","支"]
[null,"【20B","Q235","12米","支"]
[null,"工14","Q235","9米","支",66]
[null,"工16","Q235","12米","支",24]
[null,"工20A","Q235","12米","支"]
[null,"工18B","Q235","12米","支",60]
[null,"工25A","Q235","12米","支"]
[null,"H350*175","Q235","12米","支"]
[null,"H396*199","Q235","12米","支"]
[null,"口50*3","Q235","6米","支",23]
[null,"口40*3","Q235","6米","支",236]
[null,"口30*2","Q235","6米","支"]
[null,"42*3","Q235","6米","支",220]
[null,"76*6","Q235","6米","支",98]
[null,"114*5","Q235"," ","米",42]
[null,"L90*56*6","Q235","6米","支"]
[null,"L75*8","Q235","6米","支"]
[null,"L50*5","Q235","6米","支",6]
[null,"L80*80*8","Q235","6米","支",45]
[null,null,"Q235","9米","支"]
[null,"L100*100*10","Q235","9米","支"]
[null,null,"Q235","6米","支",42]
["以上报价内容为（不可更改无二次报价机会）：1、国标货、泰安满庄提货或送到、过磅含税价；2、付款方式为货到需方收货后付款；3、收货方式按照需方过磅重量（磅差千分之一以内）电汇结算；4、结算前需提供材质书、购销合同、收据、发票等相关凭据；5、供货周期为三日内到全；6、本次报价请各报价单位按照自己公司优势选着性报价，同时允许多个包件同时报价，我公司按照单项低价选择中标。"]
["本次报价有效期为：       日内（报价单位必填）       ",{"$nulls":7},"报价单位（盖章）："]
[{"$nulls":8},"报价时间："]
[{"$nulls":8},"报价人："]
[{"$nulls":8},"联系电话："]